• Fabricante y modelo de la computadora.

PROCESSOR: Intel Core i5-8265U @ 3.90GHz

Core Count: 4

Thread Count: 8

Extensions: SSE 4.2 + AVX2 + AVX + RDRAND + FSGSBASE

Cache Size: 6144 KB

Microcode: 0xca

Scaling Driver: intel\_pstate powersave

GRAPHICS: Intel UHD 3GB

Frequency: 1100MHz

OpenGL: 4.6 Mesa 19.3.2

Display Driver: intel 2.99.917

Screen: 1920x1080

MOTHERBOARD: WHL Doc\_WC

BIOS Version: V1.12

Chipset: Intel Cannon Point-LP

Audio: Realtek ALC255

Network: Realtek RTL8111/8168/8411 + Qualcomm Atheros QCA6174 802.11ac

MEMORY: 8192MB

DISK: 960GB KINGSTON SA400S3

File-System: ext4

Mount Options: discard noatime rw

Disk Scheduler: MQ-DEADLINE

OPERATING SYSTEM: ManjaroLinux 18.1.5

Kernel: 5.4.14-2-MANJARO (x86\_64)

Desktop: Xfce 4.14

|  |  |
| --- | --- |
| Prueba | Resultado |
| GZIP Compression | 82.45 |
| DCRAW | 73.32 |
| FLAC Audio Encoding | 13.63 |
| GnuPG | 22.33 |
| MAFFT | 9.424 |
| Timed MrBayes Analysis | 9.424 |
| Timed PHP Compilation | 205.41 |
| REDIS\*Test: LPOP | 1233578.08 |
| Test: SADD | 944686.89 |
| Test: LPUSH | 737895.46 |
| Test: GET | 1107833.15 |
| Test: SET | 864141.66 |